**Setting up the Nano on a Mac for Internet**

Make sure Airport is turned off and Ethernet is selected in Network Preferences!!

1. Open up Network Preferences

2. Set Configure IPv4 to Manually

3. Set IP Address to 192.168.1.28

4. Set Subnet Mask to 255.255.255.0

5. Apply

6. Open Safari and enter 192.168.1.20 in the address window

 Login UBNT P/Code UBNT

7. Open ‘wireless’ page and press 'Select'

8. Select the best suited signal, click 'Select' (and that window closes)

9. Click on 'Change at the bottom of the page and 'Apply' & 'Discard' appear at the top .

10. Click on 'Apply'

11. Go back to Network Preferences and change 'Configure IPv4' from Manually to 'Using DHCP'

Give it several seconds and the IP Address, Subnet Address, Router & DNS Server addresses should appear. If they do you will have a green light in the Ethernet window. YOU ARE CONNECTED TO THE INTERNET.

The Bigpond IP Address is 10.0.0.2